Linux version:
Add to your udev:
SUBSYSTEM=="usb", ATTR{idVendor}=="02ab", ATTR{idProduct}=="0031", MODE="0666"
or run as root


Windows version:
mmpluslogreader.exe - run to download log files from MM+ (csv and kml)

Changelog:

Firmware 2.03d 
- added silent start mode (press SW3 - to start device widthout sound),
- improved GPS logging data,


Flasher 1.02b
- added waiting for ENTER after program exit (in Windows),


LogReceiver 1.06a 
- Improved generating KML,
- Added time from log start at first position in CSV file,
- Added remember position function in rows when GPS signal is lost,
- Add waiting for ENTER after program exit ( in Windows ),
- some minor bug fixex,

