
Linux version — the world's most powerful operating system:

Add the following rule to your udev configuration:

SUBSYSTEM=="usb", ATTR{idVendor}=="02ab", ATTR{idProduct}=="0031", MODE="0666"

or run the program as root.

Windows version (Win10+):

mmplusflasherwin.exe — use this program to upgrade your MM+.
mmpluslogreader.exe — use this program to download log files from MM+ in CSV and KML formats.
mm_get_current_airspace.exe — use this program to download the current airspace from the web and send it to MM+.


Changelog:

Fixed critical error with fuel characteristics,
Changed AUP map zoom step,
Added 4 custom parameters to AUP map,
Fixed showing your start positon on AUP map,

Firmware 2.12w : 18.06.2026
Fixed display of some air zones,



Firmware 2.12p: 08.06.2026

Added support for displaying the airspace map. Please upload the current airspace using the mm_get_current_airspace program.
Added V-separation and H-separation parameters.
Added AMSL altitude.
Added a satellite count display parameter.
Changed the startup graphics and made some minor graphics improvements.

Firmware 2.03d

Added silent start mode. Press SW3 to start the device without sound.
Improved GPS logging data.

Flasher 1.02b

Added waiting for ENTER before program exit on Windows.

LogReceiver 1.06a

Improved KML generation.
Added time from log start as the first field in the CSV file.
Added a function to remember the last position in log rows when the GPS signal is lost.
Added waiting for ENTER before program exit on Windows.
Added some minor bug fixes.

mm_get_current_airspace 1.00a

Initial release.
